S-Index

A B C D E F G H I K L M N O P Q R S T U V W

## S

selectAlignment(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select alignment ESC a n
selectAlignment(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Select alignment ESC a n
selectAlignment(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select aligment ESC a n
selectBmpModel(int, int, int, byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select the bitmap mode ESC * m nL nH d1 d2...dk
selectBmpModel(int, int, int, byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Select the bitmap mode ESC * m nL nH d1 d2...dk
selectBmpModel(int, int, int, byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Select the bitmap mode ESC * m nL nH d1 d2...dk
selectCharacterCodePage(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select character codepage ESC t n
selectCharacterCodePage(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select character codepage ESC t n
selectCharacterCodePage(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select character codepage ESC t n
selectCharacterSize(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select a character size GS ! n
selectCharacterSize(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select character size GS ! n
selectChineseCharModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select chinese-char model FS &
selectChineseCharModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set Chinese Character Model FS &
selectChineseCharModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select chinese-char model FS &
selectCutPagerModerAndCutPager(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select Cut Pager Moder And CutPager GS V m
selectCutPagerModerAndCutPager(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select Cut Pager Moder And CutPager GS V m n
selectCutPagerModerAndCutPager(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select the model of cutpage and cut the pager GS V m
selectCutPagerModerAndCutPager(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select cut paper model and cut paper GS V m n
selectFont(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select Font ESC M n
selectFont(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Select Font ESC M n
selectFont(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Select Font ESC M n
selectHRICharacterPrintPosition(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select HRI character of barcode position to print GS H n HRI is the explanation of the barcode content GS H n
selectHRICharacterPrintPosition(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select HRI character of barcode position to print GS H n HRI is the explanation of the barcode content GS H n
selectHRIFont(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select HRI font type for the barcode content GS f n
selectHRIFont(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select HRI font type for the barcode content GS f n
selectInternationalCharacterSets(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select international character sets ESC R n
selectInternationalCharacterSets(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select international character set ESC R n
selectInternationalCharacterSets(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select international character set ESC R n
selectOrCancelBoldModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select or cancel the bold model ESC E n
selectOrCancelBoldModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Select or cancel the bold model ESC E n
selectOrCancelBoldModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Select or cancel the bold model ESC E n
selectOrCancelChineseCharDoubleWH(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select or cancel chinese double width and height FS W n
selectOrCancelChineseCharDoubleWH(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select or cancel chineseChar double width and height FS W n
selectOrCancelChineseCharDoubleWH(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select or cancel chinese double width and height FS W n
selectOrCancelChineseCharUnderLineModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select or cancel chinese-char underline model FS - n
selectOrCancelChineseCharUnderLineModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select Or Cancel Chinese Char UnderLine Model FS - n
selectOrCancelChineseCharUnderLineModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select or cancel chinese-char underline model FS - n
selectOrCancelConvertPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select or cancel convert print model ESC { n
selectOrCancelConvertPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select or cancel convert print model ESC { n
selectOrCancelConvertPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select or cancel convert print model ESC { n
selectOrCancelCW90(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select or cancel 90 degrees clockwise This command is available only in page mode ESC V n
selectOrCancelCW90(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select or cancel 90 degrees clockwise this command only effect in the page model ESC V n
selectOrCancelDoubelPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select or cancel double print mode ESC G n
selectOrCancelDoubelPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Select or cancel double print mode ESC G n
selectOrCancelDoubelPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Select or cancel double print mode ESC G n
selectOrCancelInvertPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select or cancel invert print mode GS B n
selectOrCancelInvertPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select or cancel invert print model GS B n
selectOrCancelUnderlineModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select or cancel underline mode ESC-n
selectOrCancelUnderlineModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Select or cancel underline mode ESC-n
selectOrCancelUnderlineModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Select or cancel underline mode ESC-n
selectOrCancelUnidirectionPrint(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select or cancel unidirection print ESC U n
selectOrCancleCustomChar(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Select or cancel user-defined characters ESC % n
selectOrCancleCustomChar(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select or cancle custom char ESC % n
selectOrCancleCustomChar(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select or cancel custom-char ESC % n
selectPageModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select page model ESC L
selectPrintColor(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select print color ESC t n
selectPrintDirectionUnderPageModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select the print direction under pager model ESC T n
selectPrinter(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select priner ESC=n
selectPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  select print model ESC £¡n
selectPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select print mode ESC £¡n
selectPrintModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select the print model ESC £¡n
selectPrintTransducerOutPutPageOutSignal(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select printer transducer output page out Signal ESC c 3 n
selectPrintTransducerOutPutPageOutSignal(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select print transducer output pageout signal ESC c 3 n
selectPrintTransducerStopPrint(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  select printer transducer stop print ESC c 4 n
selectPrintTransducerStopPrint(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select print transducer stop to print ESC c 4 n
selectStandardModel() - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  select standar model ESC S
selfTest() - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  At this command, the printer will print out the printer information SELFTEST [page]
selfTest(String) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  At this command, the printer will print out the printer information SELFTEST [page]
sendRealtimestatus(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  send real time status DLE EOT n
sendRealtimestatus(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  send real-times status DLE EOT n
setAbsolutePositionUnderPageModel(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set absolute position under page model GS $ nL nH
setAbsolutePrintPosition(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Set the absolute print position ESC $ nL nH
setAbsolutePrintPosition(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set absolutely print position ESC $ nL nH
setBarcodeHeight(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  set barcode height GS h n
setBarcodeHeight(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set barcode height GS h n
setBarcodeWidth(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  set barcode width GS w n
setBarcodeWidth(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set barcode width GS w n
setBlackPositionRecord(int, int, int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set black position record GS ( F pL pH a m nL nH
setCharRightSpace(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  seting the right side space of the character string ESC SP n
setCharRightSpace(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set char right space
setCharRightSpace(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set char right side space
setChineseCharacterModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  set chinese-char model FS ! n
setChineseCharacterModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set Chinese Character Model FS ! n
setChineseCharacterModel(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set chinese-char model FS ! n
setChineseCharLeftAndRightSpace(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  setting chinese character left and right space FS S n1 n2
setChineseCharLeftAndRightSpace(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Set the spacing Chinese characters characters.
setChineseCharLeftAndRightSpace(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  setting chinese character left and right space FS S n1 n2
setConnectWaitTime(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set the reconnect time GS z 0 t1 t2
setDefultLineSpacing() - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Set the default line spacing ESC 2 about 3.75mm
setDefultLineSpacing() - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  Set the default line spacing ESC 2 About 3.75mm
setDefultLineSpacing() - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Set the default line spacing ESC 2 About 3.75mm
setHorizontalAndVerticalMoveUnit(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  setting the positon of content horizontal and vertical move GS P x y
setHorizontalAndVerticalMoveUnit(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  setting the positon of content horizontal and vertical move GS P x y
setHorizontalmovementPosition(byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  Set the horizontal movement position ESC D n1...nk NUL;
setHorizontalmovementPosition(byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set horizontal movement position ESC D n1...nk NUL;
setHorizontalmovementPosition(byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set horizontal movement position ESC D n1...nk NUL;
setLeftSpace(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  set left space GS L nL nH
setLeftSpace(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set left space GS L nL nH
setLineSpaceing(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  set line spaceing ESC 3 n
setLineSpaceing(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  line-height ESC 3 n
setLineSpaceing(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  line-height ESC 3 n
setOrderLength(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set Order Length ESC ~ nL nH
setPrintAreaUnderPageModel(int, int, int, int, int, int, int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set print area under page model ESC W xL xH yL yH dxL dxH dyL dyH
setPrintAreaWidth(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  setting the width of print area GS W nL nH
setPrintAreaWidth(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  setting the width of print area GS W nL nH
setRelativeHorizontalPrintPosition(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  set relative horizontal print position Please refer to the details of programming instruction manual ESC \ nL nH
setRelativeHorizontalPrintPosition(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set relative horizontal print position please refer to the details of programming instruction manual ESC \ nL nH
setRollBackLength(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  set roll back length length= n¡Á0.1764 mm ESC ^ n
SetsTheErrorCorrectionLevelForPDF417(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Sets the error correction level for PDF417 symbols.
SetsTheErrorCorrectionLevelForQRCodeSymbol(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Sets the error correction level for QRCode symbol.
SetsTheModuleHeightForPDF417(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Sets the module height to [(module width) ¡Á n].
SetsTheModuleWidthOfPDF417(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Sets the module width of one PDF417 symbol to n dots.
SetsTheNumberOfColumnsOfTheDataAreaForPDF417(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Sets the number of columns of the data area for PDF417 GS ( k p L p H cn fn n (fn = 65) (p L + p H ¡Á 256) = 3 (p L = 3, p H = 0) cn = 48 fn = 65
SetsTheNumberOfRowsOfTheDataAreaForPDF417(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Sets the number of rows of the data area for PDF417 GS ( k p L p H cn fn n (fn = 66) (p L + p H ¡Á 256) = 3 (p L = 3, p H = 0) cn = 48 fn = 66
SetsTheSizeOfTheQRCodeSymbolModule(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Sets the size of the QRCode symbol module to [n dots ¡Á n dots] GS ( k p L p H cn fn n (fn = 67) Hex 1D 28 6B p L p H cn fn n [Range] p L = 3, p H = 0 cn = 49 fn = 67 1<=n<=16 [Default] n = 3
setVerticalRelativePositionUnderPageModel(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  set vertical relative under page model GS \ nL nH
shift(int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command moves the label¡¯s vertical position.
sizeBydot(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command defines the label width and length.
sizeByinch(double, double) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command defines the label width and length.
sizeBymm(double, double) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command defines the label width and length.
sound(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command controls the sound frequency of the beeper.
SpecifiesOrCancelsVariousPDF417SymbolOptions(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Specifies or cancels various PDF417 symbol options GS ( k p L p H cn fn m (fn = 70) [Range] (p L + p H ¡Á 256) = 3 (p L = 3, p H = 0) cn = 48 fn = 70 m = 0, 1 [Default] m = 0
SpecifiesTheModeForMaxiCodeSymbol(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Specifies the mode for MaxiCode symbol GS ( k p L p H cn fn n (fn = 65) Hex 1D 28 6B p L p H cn fn n [Range] p L = 3, p H = 0 cn = 50 fn = 65 50 ¡Ü n ¡Ü 54 [Default] n = 50
SpecifiesTheModeForQRCodeSymbolByn1(int) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Specifies the mode for QRCode symbol by n1; GS ( k p L p H cn fn n1 n2 (fn = 65); Hex 1D 28 6B p L p H cn fn n1 n2; [Range] p L = 4, p H = 0; cn = 49; fn = 65; n1 = 49, 50; n2 = 0; [Default] n1 = 50; n2 = 0
speed(double) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command defines the print speed SPEED n
startOrStopMacrodeFinition() - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  start or stop macrode finition GS £º
StoresSymbolDataInItheMaxiCodeSymbolStorageArea(int, int, byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Stores symbol data (d1¡dk) in the MaxiCode symbol storage area.
StoresSymbolDataInThePDF417SymbolStorageArea(int, int, byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Stores symbol data (d1...dk) in the PDF417 symbol storage area.
StoresSymbolDataInTheQRCodeSymbolStorageArea(int, int, byte[]) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  Stores symbol data (d1¡dk) in the QRCode symbol storage area.
strTobytes(String) - Static method in class net.posprinter.utils.DataForSendToPrinterPos58
  string to byte[]
strTobytes(String) - Static method in class net.posprinter.utils.DataForSendToPrinterPos76
  string to byte[]
strTobytes(String) - Static method in class net.posprinter.utils.DataForSendToPrinterPos80
  string to byte[]

A B C D E F G H I K L M N O P Q R S T U V W